From 5e0be7687ec517fb19ff24c4b59f972b80d3f0de Mon Sep 17 00:00:00 2001
From: jaseg <git-bigdata-wsl-arch@jaseg.de>
Date: Tue, 13 Apr 2021 15:13:34 +0200
Subject: Censor author-identifying info for double-blind peer review

---
 paper/rotohsm_paper.tex | 15 ++++++++++++---
 1 file changed, 12 insertions(+), 3 deletions(-)

(limited to 'paper/rotohsm_paper.tex')

diff --git a/paper/rotohsm_paper.tex b/paper/rotohsm_paper.tex
index 8c24274..a09fd3a 100644
--- a/paper/rotohsm_paper.tex
+++ b/paper/rotohsm_paper.tex
@@ -1,4 +1,4 @@
-\documentclass[nohyperref]{iacrtrans}
+\documentclass[nohyperref,submission]{iacrtrans}
 \usepackage[T1]{fontenc}
 \usepackage[
     backend=biber,
@@ -13,6 +13,15 @@
 \usepackage{eurosym}
 \usepackage{wasysym}
 \usepackage{amsthm}
+\usepackage{censor}
+
+\makeatletter
+\@ifclasswith{iacrtrans}{submission}{
+    \newcommand{\censorIfSubmission}[1]{\censor{#1}{\scriptsize[Author information removed for double-blind peer review]}}
+}{
+    \newcommand{\censorIfSubmission}[1]{#1}
+}
+\makeatother
 
 \usepackage[binary-units]{siunitx}
 \DeclareSIUnit{\baud}{Bd}
@@ -508,7 +517,7 @@ part of the system once per revolution, so we designed the longituninal PCBs as
 Our proof-of-concept security mesh covers a total of five interlocking mesh PCBs (Figure~\ref{mesh_gen_sample}). A sixth
 PCB contains the monitoring circuit and connects to these mesh PCBs.  To speed up design iterations, we automated the
 generation of this security mesh through a plugin for the KiCAD EDA
-suite\footnote{\url{https://blog.jaseg.de/posts/kicad-mesh-plugin/}}.  Figure~\ref{mesh_gen_viz} visualizes the mesh
+suite\footnote{\censorIfSubmission{\url{https://blog.jaseg.de/posts/kicad-mesh-plugin/}}}.  Figure~\ref{mesh_gen_viz} visualizes the mesh
 generation process. First, the target area is overlaid with a grid. Then, the algorithm  produces a randomized tree
 covering the grid.  Finally, individual mesh traces are traced according to a depth-first search through this tree.
 We consider the quality of the plugin's output sufficient for practical applications.  Together with FreeCAD's KiCAD
@@ -737,6 +746,6 @@ secure hardware.
     \center{This is version \texttt{\input{version.tex}\unskip} of this paper, generated on \today. The git repository
     can be found at:}
 
-    \center{\url{https://git.jaseg.de/rotohsm.git}}
+    \center{\censorIfSubmission{\url{https://git.jaseg.de/rotohsm.git}}}
 }
 \end{document}
-- 
cgit 

